**Angle bars cut and welded**

Angle bar were measured, cut and welded according to the master plan.

**Wheels welded**

Caster wheels welded and put as is.

**Door frame welded**

Angle were measured, cut and welded in shape for door. Hinges were welded, door were installed.

**Door catchers installed**

Door catches were welded and installed.

**Circuit chamber and sanitation chamber divider welded and installed**

angle bar were measured, cut and welded in shape, galvanized mesh welded into the shape.

**Galvanized steel wall added**

Galvanized steel wall welded.

**Handlebar and door knob installed**

Aluminum handlebar and door knob installed via screw.

**Bosny spray paint no. 40 white sprayed , 6 cans**

Spray painted white the frame.

**Clear coat mr. do it spray paint sprayed , c-01**

Put a clear coat to the frame.

**Glass wall added**

¼ inch thick glass wall added to the door frame.